
Logfile 5/13/19





z-velocity plot (need to close of that part of the stove body evidently)

I believe the fuel is being improperly assigned to the top blocks. The secondary air inlet is ejecting fuel out of the domain in the front-back direction. Must be a mistake in how the boundary conditions are written.



--Stove body = missing some faces

--Looks like primary air is also included in stove body